### CArclib::ArcSetDhcpIp

The ArcSetDhcpIp method updates DHCP function and static IP address of the RAID subsystem.

virtual ARC_STATUS ArcSetDhcpIp ( unsigned char bDhcpMode, unsigned char *szStaticIp );

#### Parameters:

[IN]

bDhcpMode:

Value | Meaning
0 | DHCP function disabled
1 | DHCP function enabled

szStaticIp: Null-terminated character string representing a number expressed in the Internet standard "."

(dotted) notation, format: "xxx.xxx.xxx.xxx" ex: 192.168.001.100

#### Return Values

This method returns the ARC_STATUS.

#### Note:

If the DHCP function disabled, the RAID subsystem use the static IP address.

Password required if password enabled, use ArcChkPassword member function to validate the password.