### CArclib::ArcSetMacAddr

The ArcSetMacAddr method updates the RAID subsystem MAC (M edia Access Control) address if Ethernet supported.

virtual ARC_STATUS ArcSetMacAddr ( char *MacAddress );

#### Parameters:

[IN]

MacAddress: An array contains MAC address.

#### Return Values

This method returns the ARC_STATUS.

#### Note:

The length of MacAddress must == 6 bytes.

Example of input MAC address:

char mac[6] = { 0x00, 0x04, 0xD9, 0x60, 0x00, 0x00 }