### CArclib::ArcSetTermPort

The ArcSetTermPort method updates COM port settings of the RAID subsystem.

virtual ARC_STATUS ArcSetTermPort ( unsigned char nPort, unsigned char nBaudRate, unsigned char nStopBit );

#### Parameters:

[IN]

nPort:

Value | Meaning
0 | Terminal Port
1 | Debug Port

nBaudRate:

Value | Meaning
0 | 1200 bps
1 | 2400 bps
2 | 4800 bps
3 | 9600 bps
4 | 19200 bps
5 | 38400 bps
6 | 57600 bps
7 | 115200 bps

nStopBit:

Value | Meaning
0 | 1 stop bit
1 | 2 stop bits

#### Return Values

This method returns the ARC_STATUS.

#### Note:

There are two COM ports of the RAID subsystem, one “Terminal Setting” and the other for “Debug”.

Password required if password enabled, use ArcChkPassword member function to validate the password.