### sHwMon5010

The sHwMon5010 structure contains information about H/W monitor for ARC-5010 & ARC-6010.

typedef struct _HWMON_5010 { BYTE fans; BYTE voltages; BYTE temps; BYTE powers; WORD monFan; WORD fixed12V; WORD mon12V; WORD fixed5V; WORD mon5V; WORD fixed3_3V; WORD mon3_3V; WORD fixed1_5V; WORD mon1_5V; BYTE monCtrlTemp; BYTE monBkPlaneTemp; BYTE reserved[2]; } sHwMon5010, *pHwMon5010;

#### Members:

fans

The number of fans

Voltages

The number of voltages

temps

The number of temperatures ( only Controller & BackPlane )

powers

The number of powers

monFan

The speed of fan ( in RPM )

fixed12V

Always 12000mV (12V)

mon12V

Current voltage of 12V

fixed5V

Always 5000mV (5V)

mon5V

Current voltage of 5V

fixed3_3V

Always 3300mV (3.3V)

mon3_3V

Current voltage of 3.3V

fixed1_5V

Always 1500mV (1.5V)

mon1_5V

Current voltage of 1.5V

monCtrlTemp

Current temperature of controller (in degrees centigrade)

monBkPlaneTemp

Current temperature of backplane (in degrees centigrade)

reserved

Reserved

Requirements

Header | arclib.h
Include | arclib.h

See Also

ArcGetHWMon5010