### sCOM_ATTR

The sCOM_ATTR structure contains information about the COM port.

typedef struct sCOM_ATTR { BYTE comBaudRate; BYTE comDataBits; BYTE comStopBits; BYTE comParity; BYTE comFlowControl; } sCOM_ATTR, *pCOM_ATTR;

#### Members:

comBaudRate

Value | Meaning
0 | 1200 bps
1 | 2400 bps
2 | 4800 bps
3 | 9600 bps
4 | 19200 bps
5 | 38400 bps
6 | 57600 bps
7 | 115200 bps

comDataBits

Always 1 (8 bits)

comStopBits

Value | Meaning
0 | 1 stop bit
1 | 2 stop bits

comParity

Always 0 (no parity)

comFlowControl

Always 0 (no flow control)

Requirements

Header | arclib.h
Include | arclib.h

See Also

sSYSTEM_INFO