### sSYS_CONFIG_INFO

The sSYS_CONFIG_INFO structure contains information about the system configuration parameters.

typedef struct _SYS_CONFIG_INFO { BYTE beeper; BYTE bgtask_priority; BYTE jbod_raid; BYTE hdd_read_ahead; BYTE stagger_power_on; BYTE auto_spin_down; BYTE empty_hdd_slot_led; BYTE cpu_fan_detect; BYTE hdd_smart_status_polling; BYTE auto_activate_incomplete_raid; BYTE disk_write_cache; BYTE disk_capacity_truncation; BYTE reserved[1]; }sSYS_CONFIG_INFO, *pSYS_CONFIG_INFO;

#### Members:

Beeper

beeper setting

Value | Meaning
0 | Beeper ON
1 | Beeper OFF

bgtask_priority

background task priority setting

Value | Meaning
0 | Ultra Low(5%)
1 | Low(20%)
2 | Medium(50%)
3 | High(80%)

jbod_raid

JBOD/RAID setting

Value | Meaning
0 | RAID
1 | JBOD

hdd_read_ahead

HDD read ahead cache setting

Value | Meaning
0 | Enabled
1 | Disabled Maxtor
2 | Disabled

stagger_power_on

stagger power-on setting

Value | Meaning
0 | 0.4
1 | 0.7
2 | 1.0
3 | 1.5
4 | 2.0
5 | 2.5
6 | 3.0
7 | 3.5
8 | 4.0
9 | 4.5
10 | 5.0
11 | 5.5
12 | 6.0

auto_spin_down

auto spin down(minutes)

Value | Meaning
0 | Disabled
1 | 1
2 | 30
3 | 5
4 | 10
5 | 15
6 | 20
7 | 30
8 | 40
9 | 60

empty_hdd_slot_led

empty hdd slot LED setting

Value | Meaning
0 | ON
1 | OFF

cpu_fan_detect

cpu fan detection

Value | Meaning
0 | Enabled
1 | Disabled

hdd_smart_status_polling

hdd smart status polling

Value | Meaning
0 | Disabled
1 | Enabled

auto_activate_incomplete_raid

auto activate incomplete raid

Value | Meaning
0 | Disabled
1 | Enabled

disk_write_cache

disk write cache

Value | Meaning
0 | Auto
1 | Enabled
2 | Disabled

disk_capacity_truncation

disk capacity truncation

Value | Meaning
0 | Multiples Of 10G
1 | Multiples Of 1G
2 | No Truncation

Requirements

Header | arclib.h
Include | arclib.h

See Also

ArcGetSystemConfigInfo