### CArclib::ArcSNMP

The ArcSNMP method returns the information about SNMP OID.

virtual ARC_STATUS ArcSNMP( char *SNMPMsg, int length, char *SNMPResponse, int *ResLength );

#### Parameters:

[IN]

SNMPMsg: SNMP message with BER encoding.

length: The length of SNMPMsg

[OUT]

SNMPResponse: SNMP message returned from Raid subsystem with BER encoding.

ResLength: The length of returning SNMP message.

#### Return Values

This method returns the ARC_STATUS.

#### Note:

This method is available if sSYSTEM_INFO.gsiRs232Snmp is set to true.