### CArclib::ArcGetIdentifyString

The ArcGetIdentifyString method returns the identification string of controller.

virtual ARC_STATUS ArcGetIdentifyString ( char *szIdentifyString );

#### Parameters:

[OUT]

szIdentifyString: Pointer to an array that receives the information.

#### Return Values

This method returns the ARC_STATUS.

#### Note:

The identification string is formed with “Areca RAID Subsystem” + internal model name + firmware version.

Examples: “Areca RAID SubsystemARC-1120V1.36 2005-05-18”

The length of szIdentifyString must be >= 50 characters