### CArclib::ArcIdentifyDisk

The ArcIdentifyDisk method identifies one or more devices (disks).

virtual ARC_STATUS ArcIdentifyDisk ( DWORD nDevMask, );

#### Parameters:

[IN]

nDevMask: The devices mask represents the index of devices use to identify devices,

Bit0 represents device0, Bit1 represents device1….and so on.

Set the nDevMask to 0 to stop the disk identifying.

Example: The mask of 0x00000010 means that identify device4.

#### Return Values

This method returns the ARC_STATUS.

#### Note:

Password required if password enabled, use ArcChkPassword member function to validate the password.